**APPLICATIONS**

* Medical devices
* IoT
* Portable devices
* Wearables

**FUNCTIONAL BLOCK DIAGRAM**





**DESCRIPTION**

The PMT 100 is a medium 40W wireless power solution without a microcontroller on the receiver side and can be tailored to fit specific product requirements based on SmartInductive™ Technology. The solutions supply the power, magnetics, and interface to meet customer product requirements. The solutions deliver pinnacle flexibility, safety, and cost-efficiency for a 100% wireless life.

**FEATURES**

* Up to 40W wireless power transfer
* Up to 15mm coil to coil distance
* Up to 15mm lateral misalignment
* Advanced battery charging algorithm
* Optimizing power transfer efficiency in low power mode
* Software based DC-to-DC functionality
* Operation frequency 100-300KHz
* Cost-effective: Software-based MCU-less Rx solution designed for small device charging

***Powercast products and technology are covered by one or more patents with other patents pending. All patent and trademark information can be found at*** [***http://www.powercastco.com/IP/***](http://www.powercastco.com/IP/)***.***

**SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **Feature** | **Specification** | **Note** |
| **Wireless Power Transfer** |
| Coil size (Symmetric Rx, Tx, coil) | 20mm/30mm/40mm | Optional customization |
| Max charge power | 40W | Battery charging/fixed voltage |
| Coil to coil distance\* | 15mm (40mm coil)10mm (30mm coil)7mm (20mm coil) | SmartInductive™Technology mid-range coupling |
| Coil lateral misalignment (X/Y)\* | 15mm (40mm coil)10mm (30mm coil)7mm (20mm coil) | SmartInductive™Technology mid-range coupling |
| Efficiency | >90% | Peak end-to-end |
| Operation Frequency | 100KHz-300KHz |  |
| **Battery Management** |
| Battery charging | CCCV | 1-2 li-lon cells |
| Battery voltage | Up to 30V on Rx module  | Software controlled DCDC over the inductive link |
| Maximum charge current | 2A |  |
| Fuel gauging |  | Software algorithm |
| Battery protection | OV, OC | Software algorithm |
| **PCB Dimensions** |
| PCB Dimensions | 15 x 15mm | Can be customized |
| **Environmental** |
| Operating  | 0°C ~ 70°C |  |
| Storage | -40°C ~ 85°C |  |

\*Coil distance and lateral misalignment are coil size dependent



**Powercast Corporation**

620 Alpha Drive

Pittsburgh, PA, USA 15238

[www.powercastco.com](http://www.powercastco.com)

contact@powercastco.com

+1 (412)-455-5800

**CRITICAL APPLICATIONS DISCLAIMER**

POWERCAST PRODUCTS (INCLUDING HARDWARE AND/OR SOFTWARE) ARE NOT DESIGNED OR INTENDED TO BE FAIL-SAFE, FAULT TOLERANT OR FOR USE IN ANY APPLICATION THAT COULD LEAD TO DEATH, PERSONAL INJURY OR SEVERE PROPERTY OR ENVIRONMENTAL DAMAGE (INDIVIDUALLY AND COLLECTIVELY, “CRITICAL APPLICATIONS”), SUCH AS LIFE-SUPPORT OR SAFETY DEVICES OR SYSTEMS, CLASS III MEDICAL DEVICES, NUCLEAR FACILITIES, APPLICATIONS THAT AFFECT CONTROL OF A VEHICLE OR AIRCRAFT, APPLICATIONS RELATED TO THE DEPLOYMENT OF AIRBAGS, OR ANY OTHER CRITICAL APPLICATIONS. CUSTOMER AGREES, PRIOR TO USING OR DISTRIBUTING ANY SYSTEMS THAT INCORPORATE POWERCAST PRODUCTS, TO THOROUGHLY TEST THE SAME FOR SAFETY PURPOSES. CUSTOMER ASSUMES THE SOLE RISK AND LIABILITY OF ANY USE OF POWERCAST PRODUCTS IN CRITICAL APPLICATIONS, SUBJECT ONLY TO APPLICABLE LAWS AND REGULATIONS GOVERNING LIMITATIONS ON PRODUCT LIABILITY.

Powercast warrants its products in accordance with Powercast’s standard warranty available at [www.powercastco.com/terms-conditions](http://www.powercastco.com/terms-conditions)

## IMPORTANT NOTICES

Information furnished by Powercast Corporation (Powercast) is believed to be accurate and reliable. However, no responsibility is assumed by Powercast for its use, nor for any infringements of patents or other rights of third parties that may result from its use.

Specifications are subject to change without notice.

No license is granted by implication or otherwise under any patent or patent rights of Powercast. Trademarks and registered trademarks are the property of their respective owners.